**Assignment -4** Data Publish to IOT Device

|  |  |
| --- | --- |
| Assignment Date | 27 October 2022 |
| Student Name | ASIKA BANU |
| Student Roll Number | 110119104012 |
| Maximum Marks | 2 Marks |

# Question-1:

Write code and connections in wokwi for ultrasonic sensor. Whenever distance is less 100 cms send “alert” to ibm cloud and display in device recent events.

# Solution:

#include <WiFi.h>//library for wifi #include <PubSubClient.h>//library for MQtt

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "qxm592"//IBM ORGANITION ID

#define DEVICE\_TYPE "weather\_device"//Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "weather\_today"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "jwSiUN+qppnF1\*xTRa" //Token String data3;

float dist;

//-------- Customise the above values --------

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";// Server Name char publishTopic[] = "iot-2/evt/Data/fmt/json";// topic name and type of event perform and format in which data to be send

char subscribetopic[] = "iot-2/cmd/test/fmt/String";// cmd REPRESENT command type AND COMMAND IS TEST OF FORMAT STRING

char authMethod[] = "use-token-auth";// authentication method char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;//client id

// -

WiFiClient wifiClient; // creating the instance for wificlient

PubSubClient client(server, 1883, callback ,wifiClient); //calling the predefined client id by passing parameter like server id,portand wificredential

int LED = 4; int trig = 5; int echo = 18; void setup()

{

**Serial**.begin(115200); pinMode(trig,OUTPUT); pinMode(echo,INPUT); pinMode(LED, OUTPUT); delay(10); wificonnect(); mqttconnect();

}

void loop()// Recursive Function

{

digitalWrite(trig,LOW); digitalWrite(trig,HIGH); delayMicroseconds(10); digitalWrite(trig,LOW);

float dur = pulseIn(echo,HIGH); float dist = (dur \* 0.0343)/2; **Serial**.print ("Distancein cm"); **Serial**.println(dist);

PublishData(dist); delay(1000);

if (!client.loop()) { mqttconnect();

}

}

/\*.....................................retrieving to

Cloud. \*/

void PublishData(float dist) { mqttconnect();//function call for connecting to ibm

/\*

creating the String in in form JSon to update the data to ibm cloud

\*/

String object; if (dist <100)

{

digitalWrite(LED,HIGH); **Serial**.println("object is near"); object = "Near";

}

else

{

digitalWrite(LED,LOW); **Serial**.println("no object found"); object = "No";

}

String payload = "{\"distance\":"; payload += dist;

payload += "," "\"object\":\""; payload += object;

payload += "\"}";

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish ok");// if it sucessfully upload data on the cloud then it will print publish ok in Serial monitor or else it will print publish failed

} else {

**Serial**.println("Publish failed");

}

}

void mqttconnect() {

if (!client.connected()) { **Serial**.print("Reconnecting client to "); **Serial**.println(server);

while (!!!client.connect(clientId, authMethod, token)) {

**Serial**.print("."); delay(500);

}

initManagedDevice();

**Serial**.println();

}

}

void wificonnect() //function defination for wificonnect

{

**Serial**.println(); **Serial**.print("Connecting to ");

WiFi.begin("Wokwi-GUEST", "", 6);//passing the wifi credentials to establish the connection

while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.println(""); **Serial**.println("WiFi connected"); **Serial**.println("IP address: "); **Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

if (client.subscribe(subscribetopic)) { **Serial**.println((subscribetopic)); **Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

}

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

**Serial**.print("callback invoked for topic: ");

**Serial**.println(subscribetopic);

for (int i = 0; i < payloadLength; i++) {

//Serial.print((char)payload[i]); data3 += (char)payload[i];

}

// Serial.println("data: "+ data3);

// if(data3=="Near")

// {

// Serial.println(data3);

// digitalWrite(LED,HIGH);

// }

// else

// {

// Serial.println(data3);


// digitalWrite(LED,LOW);


// } data3="";

}


# OUTPUT:


**OBJECT NEAR BY DEVICE:**





# OBJECT FAR AWAY FROM DEVICE:





REFERENCE:

https://wokwi.com/projects/347211841025344084